![Image description](https://github.com/nathalis/NesCat/raw/main/NESCAT_icon.png)

# NesCat 0.5

NESCAT by Nathalis
prototype version: 0.5 (c)2020
Enhanced version Nintendo Emulator for ESP32

Requirements: ESP32 WEMOS D1 MINI, ST7789 LCD, MICROSD CARD slot,
PCM5102 I2S AUDIO MODULE, OTHER PARTS...


### FEATURES:

- MicroSD card support
- 240*240 1.3" LCD ST7789 display                  
- Composite TV OUT Video PAL
- I2S AUDIO support PCM5102 module
- PS2 (USB) KEYBOARD support (wireless not work)
- huge NES ROMs up to 512kB (read from FLASH)
- PS4 DualShock BlueTooth Gamepad (experimental)

Only for personal & educational use! 

### DIAGRAM (NEW)
![Image description](https://github.com/nathalis/NesCat/raw/main/PCB/SCHEMATIC.png)
![Image description](https://github.com/nathalis/NesCat/raw/main/PCB/BOARD.png)


### IMAGES:

![Image description](https://github.com/nathalis/NesCat/raw/main/Images/001.jpg)
![Image description](https://github.com/nathalis/NesCat/raw/main/Images/002.jpg)
![Image description](https://github.com/nathalis/NesCat/raw/main/Images/003.jpg)
![Image description](https://github.com/nathalis/NesCat/raw/main/Images/004.jpg)
![Image description](https://github.com/nathalis/NesCat/raw/main/Images/005.jpg)
![Image description](https://github.com/nathalis/NesCat/raw/main/Images/006.jpg)
![Image description](https://github.com/nathalis/NesCat/raw/main/Images/007.jpg)
![Image description](https://github.com/nathalis/NesCat/raw/main/Images/008.jpg)
![Image description](https://github.com/nathalis/NesCat/raw/main/Images/009.jpg)
![Image description](https://github.com/nathalis/NesCat/raw/main/Images/010.jpg)
![Image description](https://github.com/nathalis/NesCat/raw/main/Images/011.jpg)
![Image description](https://github.com/nathalis/NesCat/raw/main/Images/012.jpg)


